======================================================
License Agreement for Fuji Xerox PCL 6 Print Driver
======================================================

1. PROPRIETARY RIGHTS: Title, ownership rights, and intellectual
   property rights in the SOFTWARE shall remain in Fuji Xerox and its
   third party suppliers.  You have no rights in the SOFTWARE except
   as expressly granted in accordance with this agreement.
   
2. LICENSE:  Under this agreement, you are granted a non-exclusive
   license to use the SOFTWARE for the purpose of using with
   compatible Fuji Xerox products in your country.  You are
   not permitted to (1) assign, sublicense, sell, rent, lease, convey,
   or transfer the SOFTWARE to any third party by any tangible media
   such as floppy disk, magnetic tape, or CD-ROM, (2) distribute the
   SOFTWARE on a network or by a telephone line available to the
   public or (3) alter, modify, decompile, disassemble, reverse
   engineer, or create derivative works based on the whole or any
   part of the SOFTWARE.
   If any direction on usage or restriction for the SOFTWARE is
   expressly specified in this web site, you are required to follow
   such direction. 
   
3. TERM: This agreement is effective upon installing the SOFTWARE
   until you terminate the agreement by destroying the SOFTWARE.
   This agreement will also terminate if you fail to abide by any
   terms of this agreement.  In case of termination, you must
   promptly destroy the SOFTWARE.
   
4. LIMITED WARRANTIES: THE SOFTWARE IS SUPPLIED STRICTLY ON AN 'AS IS'
   BASIS WITHOUT WARRANTY OF ANY KIND, EITHER EXPRESSED OR IMPLIED,
   INCLUDING BUT NOT LIMITED TO ANY WARRANTY OF MERCHANTABILITY OR
   FITNESS FOR A PARTICULAR PURPOSE, WITH RESPECT TO THE SOFTWARE.
   YOU ARE RESPONSIBLE FOR CHOOSING, MAINTAINING AND MATCHING OTHER
   HARDWARE AND SOFTWARE COMPONENTS IN COMBINATION OF THE SOFTWARE.
   IN NO EVENT, SHALL FUJI XEROX, FUJI XEROX CHANNEL PARTNERS,
   AUTHORIZED DEALERS AND THEIR THIRD PARTY SUPPLIERS BE LIABLE FOR
   ANY LOSS OR DAMAGE INCLUDING INCIDENTAL OR CONSEQUENTIAL LOSS OR
   DAMAGE, ARISING FROM USE OF OR INABILITY TO USE SOFTWARE, OR ANY
   MODIFICATION OF THE SOFTWARE.  
   
5. EXPORT CONTROL: You are not allowed to export the SOFTWARE in part
   or whole, directly or indirectly, in violation of any restrictions,
   laws or regulations imposed by the government of your country or
   any other relevant countries, and are required to obtain necessary
   approval prior to exporting the SOFTWARE.


-----------------------------------------------------------------------
FX DocuCentre-III 3007/2007 PCL 6
Print Driver for Microsoft(R) Windows(R) XP x64 Edition,
Microsoft(R) Windows Server(R) 2003 x64 Edition,
Microsoft(R) Windows Server(R) 2008 x64 Edition,
Microsoft(R) Windows Vista(R) x64 Edition,
Microsoft(R) Windows(R) 7 x64 Edition,
Microsoft(R) Windows Server(R) 2008 R2,
Microsoft(R) Windows(R) 8 x64 Edition,
Microsoft(R) Windows Server(R) 2012
Version 2.7.4(1/1)
July 2012

Readme
-----------------------------------------------------------------------

This document describes

  1. Requirements
  2. File Configuration
  3. Installation
  3.1. Installation on Windows(R) XP x64 Edition, Windows Server(R) 2003 x64 Edition
  3.2. Installation on Windows Vista(R) x64 Edition, Windows(R) 7 x64 Edition,
       Windows Server(R) 2008 x64 Edition
  3.3. Installation on Windows(R) 8 x64 Edition, Windows Server(R) 2012
  3.4. Uninstallation on Windows(R) XP x64 Edition, Windows Server(R) 2003 x64 Edition
  3.5. Uninstallation on Windows Vista(R) x64 Edition, Windows Server(R) 2008 x64 Edition,
       Windows(R) 7 x64 Edition, Windows Server(R) 2008 R2, Windows 8 x64 Edition,
       Windows Server(R) 2012
  4. General Comments
  5. Limitations
  6. Software Update


1. Requirements
===============

1. Please note that this print driver operates on a computer with a
   64-bit x64-based microprocessor (AMD64 or Intel EM64T) and an
   upward-compatible processor, running
   Microsoft(R) Windows(R) XP x64 Edition,
   Microsoft(R) Windows Server(R) 2003 x64 Edition,
   Microsoft(R) Windows Server(R) 2008 x64 Edition,
   Microsoft(R) Windows Vista(R) x64 Edition,
   Microsoft(R) Windows(R) 7 x64 Edition,
   Microsoft(R) Windows Server(R) 2008 R2,
   Microsoft(R) Windows(R) 8 x64 Edition,
   Microsoft(R) Windows Server(R) 2012
   English Version.


2. File Configuration
=====================
fx6shie.inf
fx6sheiu.dll
fx6sheim.dll
fx6shjdm.dll
fx6sheir.xrs
fx6shkdm.dll
fxzddmif.dll
fxzdhb32.dll
fxzdmifk.dll
fxzadc2.dll
fxzarl32.dll
fxzkhxa5.dll
fxzvup.exe
fx6she.cfg
fx6she.tbl
fx6she.chm
fxzkhf01.dll
fxzkhf01.exe
fx6she.xrs
fx6she.cdd
fx6she.ddd
fx6sie.ddd
fxzkvup.dll
fx6shie.cat


3. Installation
===============

Follow the instructions below to install PCL 6 print drivers.

Here we will install and uninstall the FX DocuCentre-III 3007 PCL 6
print driver as an example.


3.1 Installation on Windows(R) XP x64 Edition, Windows Server(R) 2003 x64 Edition
==================================================================================

(1) Click the "Start" button.  Point to "Settings" and click
    "Printers and Faxes".

(2) Double-click the "Add a printer" icon in the "Printers and Faxes" 
    dialog box, and then follow the instructions on the dialogs.

(3) If the printer is directly attached to your computer or is
    connected to the Network using the LPR protocol, choose "Local 
    printer attached to this computer" ,then click "Next>" and follow 
    the instructions from (5).Otherwise, choose "A network printer, 
    or a printer attached to another  computer".

(4) Connect to the desired printer by one of the method:
         * Perform a search in the Active Directory
         * Click "Next>" to locate the printer on the network, or
           "Connect to this printer type" button to type the name
           using the following format. 
           
           \\printserver_name\share_name

    Then follow the instructions from (10).
    If you are not familiar with the network, please consult the
    network administrator.

(5) Select the printer port where the printer device is connected
    directly, click "Next>", and go to step (7).
    If the printer is connected to the Network using the LPR protocol,
    select "Standard TCP/IP Port" of the "Create a new port:" section,
    and then click "Next>". The "Welcome to the Add Standard TCP/IP
    Printer Port Wizard" dialog box will be displayed. Click "Next>".

(6) Enter the Printer Name or IP address in the "Printer Name or IP
    Address" edit box. If you do not know the Printer Name or IP
    address, please consult the network administrator.
    The "Completing the Add Standard TCP/IP Printer Port Wizard"
    dialog box will be displayed. Click "Finish". 

(7) Click "Have Disk..." from the "Add Printer Wizard" screen.
    An "Install From Disk" screen is displayed. Specify a folder
    in which the driver files are. Then select the INF file in
    the folder and then click "OK".

(8) "FX DocuCentre-III 3007 PCL 6" appears in the dialog box. Select
    the printer and click "Next".
    If the selected printer is already installed, a message asking
    whether to replace the existing driver is displayed.
    When installing a new version of the print driver, select
    "Replace existing driver".  The older version of the driver cannot
    be deleted if it is used in an application.
    In this case, close the application. 

(9) A dialog box for specifying the printer name is displayed. 
    To change the printer name, enter any name in the "Printer name"
    box.  If other printers are installed, a message asking whether
    to make this the default printer is shown.  Click "Yes". 

(10) Specify whether to share this printer with other network users. 

(11) A dialog box specifying whether to print the test page after
     installation is shown.
     If you select "Yes", load paper in the printer and click "Next".
     Select "No" and click "Next" if you do not wish to print the test
     page. 

(12) A dialog box to confirm the settings is displayed. Click "Finish"
     after confirming the settings.

(13) A message saying that it did not pass the Windows Logo Test will
     be displayed but this does not cause functional problem. Click
     "Continue Anyway"
   
(14) The necessary files are copied and a new printer icon is created.
     If you have printed the test page, a printer test result
     confirmation message is displayed. 
     This completes the installation. 


3.2 Installation on Windows Vista(R) x64 Edition, Windows(R) 7 x64 Edition,
    Windows Server(R) 2008 x64 Edition
===========================================================================

(1) Click the "Start", select [ControlPanel], and then click [Printer] 
    on [Hardware and Sound].

    For Windows(R) 7, follows steps below
    Start > Device and Printer > Select "Add a Printer" in Device and Printer.

(2) Select [Add Printer] from the menu bar.

(3) If the printer is directly attached to your computer or is
    connected to the Network using the LPR protocol, choose " Add a local 
    printer " ,then click "Next>" and follow the instructions from (5).
    Otherwise, choose " Add a network, wireless or Bluetooth printer".

(4) Select [The printer that I want isn't listed].
    Connect to the desired printer by one of the method:
         * Perform a search in the Active Directory
         * Select "Browse for a printer" button, and then click "Next>" to 
           locate the printer on the network, or "Select a shared printer 
           by name" button to type the name using the following format. 
           
           \\printserver_name\share_name

    Then follow the instructions from (11).
    If you are not familiar with the network, please consult the
    network administrator.

(5) Select the printer port where the printer device is connected
    directly, click "Next>", and go to step (7).
    If the printer is connected to the Network using the LPR protocol,
    select "Standard TCP/IP Port" of the "Create a new port:" section,
    and then click [Standard TCP/IP port].

(6) Enter the Hostname or IP address in the "Hostname or IP
    Address" edit box. If you do not know the Hostname or IP
    address, please consult the network administrator.

(7) Click "Have Disk...." in the "Add Printer Wizard" and specify
    a folder in which the driver files are. Then select the INF
    file in the folder and then click "OK".

(8) "FX DocuCentre-III 3007 PCL 6" appears in the dialog box. Select
    the printer and click "Next".
    If the selected printer is already installed, a message asking
    whether to replace the existing driver is displayed.
    When installing a new version of the print driver, select
    "Replace the current driver".  The older version of the driver cannot
    be deleted if it is used in an application.
    In this case, close the application. 

(9) A dialog box for specifying the printer name is displayed. 
    To change the printer name, enter any name in the "Printer name"
    box.  If other printers are installed, a message asking whether
    to make this the default printer is shown.  
    Confirm that "Set as the default printer" is selected.

(10) [User Account Control] dialog will be displayed and ask if you continue 
     [Change Printing Settings]. Click [Continue]. When executing installation
     as a user other than Administrator, password for Administrator is required.

(11) Installation starts.  A message saying that Windows can't verify the 
     publisher of this driver software will be displayed but this does not 
     cause functional problem. Click "Install this driver software anyway" 
     to continue the installation.

(12) Specify whether to share this printer with other network users.

(13) A dialog box specifying whether to print the test page after installation 
     is shown. Click [Print a test page] button to print the test page.  
     Otherwise, click "Finish" if you do not wish to print the test page.


3.3 Installation on Windows(R) 8 x64 Edition, Windows Server(R) 2012
==========================================================================

(1) Go to Control Panel > "Hardware and Sound" > "Devices and Printers".

(2) Select "Add a printer" from the menu bar.

(3) Specify the printer connection.
    * For a local printer:
      Specify the local printer going through the menu displayed on Windows.
      Proceed to Step (4)
    * For a network printer:
      Specify the desired printer from the network going through the menu
      displayed on Windows.
      Contact the network administrator if you have any queries.
      If other printers are installed, a message asking whether
      to set this as the default printer is shown. Click "Yes"
      if you want to set it as a default printer.
      Proceed to step (8).

(4) Specify the printer port. Create a port if there is no output port.
    Please refer to the "Frequently Asked Questions" from our driver
    download page for the port creation method.

(5) Specify the printer model. Click "Have Disk..." to display the
    "Install From Disk" dialog box.
    Select a folder in which the driver files are. Then select the INF
    file in the folder and then click "OK".

(6) "Multi-model Print Driver 2" appears in the dialog box. Select
    the printer and click "Next".
    If the selected printer is already installed, a message asking
    whether to replace the existing driver is displayed.
    When installing a new version of the print driver, select
    "Replace the current driver".  The older version of the driver
    cannot be deleted if it is used in an application.
    In this case, close the application.

(7) A dialog box for specifying the printer name is displayed.
    To change the printer name, enter any name in the "Printer name"
    box.

(8) Installation starts.
    * "User Account Control" dialog will be displayed and ask if you
      continue "Change Printing Settings". Click "Continue".
      When executing installation as a user other than Administrator,
      password for Administrator is required.
    * The installation confirmation screen published by Fuji Xerox Co.,
      Ltd. may be displayed, but it is not a functional problem.
      Click "Install".

(9) A dialog box specifying whether to print the test page after installation
    is shown. Click "Print a test page" button to print the test page.
    Otherwise, click "Finish" if you do not wish to print the test page.

About driver deletion method 
(When using Windows Vista, Windows Server 2008, Windows 7, Windows 8 or Windows Server 2012)
-------------------------------------------------------------------------
To remove drivers from system completely, please delete drivers and driver 
package going through the following steps.
Please note that driver package can not be deleted by executing driver 
uninstall tool.

About driver installation method using plug-and-play
(When using Windows 7, Windows Server 2008 R2, Windows 8 or Windows Server 2012)"
-----------------------------------------------------
When a driver is installed using plug-and-play, it may not
be installed properly.  In such case, follow the steps below to reinstall
the driver.
     * Select "Device and Printer".
     * Right click on the printer icon in the "Device and Printer" folder,
       them, select "Properties".
       Reboot the computer in case of the icon is dimmed out.
     * Select the printer icon in the "Device Function" in "Hardware" tab,
       then, open properties dialog by clicking "Properties" button.
     * A new "Properties" dialog is opened by click "Change Settings" button.
     * Open "Driver" tab from the new "Properties" dialog box, click 
       "Update Driver","Update Driver Software" dialog will be opened.
     * Select "Browse my computer for driver software","Serch for driver 
       software in this location" specific driver files location you want to 
       install then, click "Next".
     * Click "Close" button when driver has been updated message displayed, to
       complete reinstallation.


3.4 Uninstallation on Windows(R) XP x64 Edition, Windows Server(R) 2003 x64 Edition
===================================================================================

(1) Delete the printer icon you installed in the "Printers" dialog
    box from the "Control Panel".


3.5 Uninstallation on Windows Vista(R) x64 Edition, Windows Server(R) 2008 x64 Edition,
    Windows(R) 7 x64 Edition, Windows Server(R) 2008 R2, Windows(R) 8 x64 Edition, Windows Server(R) 2012
=============================================================================

(1) For Windows Vista(R), Windows Server(R) 2008.
    * Click "Start" button, open "Control Panel", then select "Printer" in
      "Hardware and Sound".
    * Delete the printer icon in the "Printer" folder.
    * Right-click on the "Printer" folder, go to "Run as administrator" ->
      "Server Properties" and display "Print Server Properties".
    * Select the driver to be deleted on the "Driver" tab and click the
      "Remove" button.
    * Select "Remove driver and driver packages" and click "OK".
    * Reboot the computer.

(2) For Windows(R) 7, Windows Server(R) 2008 R2.
    * Click "Start" button, then select "Device and Printer".
    * Delete the printer icon in the "Device and Printer" folder.
    * Select any icon displayed in the "Printer and Fax" from inside of 
      "Device and Printer" folder, then select "Printer Server Properties". 
    * Click the button "Change Driver Settings".
    * Select the driver to be deleted on the "Driver" tab and click the
      "Remove" button.
    * Select "Remove driver and driver packages" and click "OK".
    * Driver packages may not be removed while driver is being used, retry
      after reboot the computer.
    * Reboot the computer.

(3) For Windows(R) 8, Windows Server(R) 2012.
    * Go to "Control Panel" > "Hardware and Sound" > "Devices and Printers".
    * Delete the printer icon in the "Device and Printer" folder.
    * Select any icon displayed in the "Printer" from inside of 
      "Device and Printer" folder, then select "Printer Server Properties". 
    * Click the button "Change Driver Settings".
    * Select the driver to be deleted on the "Driver" tab and click the
      "Remove" button.
    * Select "Remove driver and driver packages" and click "OK".
    * Driver packages may not be removed while driver is being used, retry
      after reboot the computer.
    * Reboot the computer.


4. General Comments
===================

(1) Close all the running applications before installing the print
    driver.

(2) Always reboot the computer after installing an upgraded version of
    the print driver.

(3) If you have deleted an older version of the print driver,
    always reboot the computer before installing the new version.

(4) Some applications provide printing options pertaining to the
    number of copies and collated copies.  Always select the printing
    options in the application unless the instructions specify
    otherwise. Use the print driver dialogs to select advanced
    options such as 2 Sided Print, Sample Set or options that are
    not available in the application.

(5) Always close the print driver dialogs and/or the application
    Print dialog box before you make any changes to the default
    settings of the print driver via the Control Panel.

(6) If your Job Offset output does not work well with the collated
    copies, you may try to deselect the "Collate" option in the
    application and check the "Collate" check box in the print
    driver.

(7) If a Fax Phonebook is not initialized or created by the current
    user, he/she may not be granted the authority to access it.
    For such inappropriate access by users, the driver will display
    an error message indicating that the default Fax Phonebook cannot
    be located or the specified Fax Phonebook cannot be recognized.
    On the other hand, if a user would like his/her Fax Phonebook to
    be accessed by other users, he/she has to specify the groups and
    users whose access he/she wants to allow, and must grant them
    at least the 'Change' permission to the Fax Phonebook data file.

(8) A fax job has to be sent separately to each recipient who is
    specified with the F-code, Password or secure send attributes.
    Otherwise, the printer always disregards the F-code, Password
    and secure send attributes when sending a fax job to multiple
    recipients.  The transmitted job is always printed directly
    at all specified destinations.

(9) If OS other than the intended OS for this driver is used on a client 
    site of shared printer, an alternate driver for each OS has to be 
    installed.
    The version of the alternate driver should correspond with the version 
    of this driver.  Otherwise, the installation of the alternate driver 
    may have some errors.
    Also, the following OS cannot be used on a client site of shared printer.
    - Any previous versions to Windows(R) XP SP2
    - Any previous versions to Windows Server(R) 2003 SP1
    - Windows(R) 2000
    If any of the above OS is used on a client site and shared printer is 
    installed, Properties of the Printers folder may not open.

(10) For the installation through the networks on Windows Vista(R),
     if you right-click on [Printer] folder, go to "Run as administrator" 
     from the menu and select [Add printer...], printer icon may not be generated.

(11) Rename a Printer Icon should comply OS file naming convention. Use Symbols or 
     special characters may incur renaming error or unexpected print driver behavior.

(12) Before installing a print driver in the Windows cluster environment, you need
     to install it on each node in the cluster.

(13) Please refer to the following chapter in case of using 
     "Uninstall print driver" on Windows Vista(R), Windows Server(R) 2008,
      Windows(R) 7, Windows(R) 8 or Windows Server(R) 2012.
     "About driver deletion method
      (When using Windows Vista, Windows Server 2008 ,Windows 7 or Windows 8)"

(14) For Plug and Play driver installation on Windows(R) 7, Windows(R) 8
     or Windows Server(R) 2012, Please refer to the following chapter.
     "About driver installation method using plug-and-play
      (When using Windows 7 or Windows 8)"

5. Limitations
==============

(1) When a printed pattern or diagram is different from what you see
    on the screen, changing the following settings may alleviate the
    problem.

    * Change the "Image Quality" setting on the "Image Options" tab.
    * Change the "Brightness" and the "Contrast" settings on the
      "Image Options" tab.
    * Set "High Speed Image Processing" on the "Advanced Settings"
      tab to "Off".
    * Set "Draw the pattern with fine lines as per the resolution"
      on the "Advanced Settings" tab to "On".
    * Change the "Resolution" setting in the "Other Settings
      (Graphics Settings)" on the "Advanced Settings" tab.
    * Change the "Halftone Print" setting in the "Other Settings
      (Graphics Settings)" on the "Advanced Settings" tab.

(2) The print layout may be changed when you change the "Image Quality"
    in the "Image Options" tab.

(3) Depending on the application, if the "Image Quality" is
    "High Resolution" or the resolution of the driver is "1200dpi",
    the size of the print data may become huge and printing cannot
    be done properly. When this happens, specify the following
    settings:

    * Specify the "Image Quality" to "Standard" in the "Image Options" tab
      or "Resolution" in the "Other Settings (Graphics Settings)" in
      the "Advanced Settings" tab to "600dpi", "300dpi" or "200dpi"

(4) When printing from the application of QuarkXpress 6.1E, if the
    "Image Quality" setting is "High Resolution" and the resolution of
    the driver is "1200dpi", the document may be printed as blank
    pages.  This issue can be avoided by changing the resolution of
    the driver to "Auto".

(5) For some applications, if a pasted image is printed at high
    resolution, the print data expands and may result in an extremely
    slow printing speed.
    The print data size of the output may be improved by changing the
    following settings of "Other Settings (Graphics Settings)" on
    the "Advanced Settings" tab.

    * Specify the "Image Compression" in the "Other Settings (Graphics
      Settings)" in the "Advanced Settings" tab to "Standard" or "Photo"
      or "Resolution" to "300dpi" or "200dpi"

(6) When printing from the application of Visio2003, if the
    "Image Quality" setting is changed from "Standard" to
    "High Resolution" before printing, data may be scaled down and
    printed in the upper left corner.  This issue can be avoided by
    setting "Image Quality" to "High Resolution" in the printer folder
    before starting the application.

(7) When doing a print job by specifying Paper Source as Auto, be
    sure to set Paper Size in the application to the Paper Size that
    the driver supports to enable the automatic paper feed feature.

(8) When using the Form Overlay feature, use form data of the same
    Paper Size, Resolution, and Image Settings as those of the
    document you want to print.  If these settings are different
    between form data and the page where the form data is incorporated,
    expected print results may not be obtained.

(9) When using Form Overlay, as some applications paint the background in
    white to print, forms with overlay may be hidden.  Such applications 
    include Internet Explorer and WordPad.

(10) With Adobe PageMaker, when this printer is specified for "Compose
     to printer", a layout may change in printing.  This issue can be
     avoided by performing the following steps;

     <1> Do not set "Compose to printer".
     <2> Change the "Margins" setting in advance in the printer folder.
     <3> Specify "Print to Edge" on the Print Area tab in advance in the
         printer folder.

(11) The print result may overlap if Multiple Up and Print Area
     [Normal] are selected when printing a document that has exceeded
     the print area of the print driver. When this happens, select
     the "Print to Edge" in the "Print Area" dialog box in the
     "Image Shift / Print Position" in the "Layout" tab.

(12) When you cancel a fax job in progress from the driver, the
     application may display a warning dialog box. It may indicate
     a printer error message, although there is no error in the
     printer. In this case, ignore the warning message and continue
     operation.

(13) To use the "Save to Mailbox" feature, a mailbox must be registered
     in advance on the printer. Refer to the machine user guide on how
     to register mailboxes.
     On FX DocuCentre-III 3007/2007, [Save to Mailbox] is available only
     when the scanner kit has been installed.

(14) Depending on the application used by the customer, blank pages
     for page adjustment will be inserted automatically according to
     the conditions like the number of copies specified when
     outputting 2 sided prints.  In this case, the blank inserts will
     be included by the application.
     The performance may be improved by changing the setting below.
     - Check "Skip Blank Pages" on "Advanced Settings" tab.

(15) Even with "Skip Blank Pages" selected, blank pages may still be
     printed in the following situations. 

     * The page contains only line feeds. 
     * The page contains only spaces. 
     * The page contains only line feeds and spaces. 
     * A white background drawing instruction is sent from the
       application. 

(16) With Microsoft(R) Word, even if "Skip Blank Pages" is specified, 
     when a blank page is included in documents, it may be output.

(17) For customers using Microsoft(R) Windows Server(R) 2000, Microsoft(R)
     Windows Server(R) 2003 or Microsoft(R) Windows Server(R) 2008 Cluster
     Environment
     <1> Use the following operating systems (32-bit version) as client:
           Microsoft(R) Windows(R) 2000
           Microsoft(R) Windows(R) XP
           Microsoft(R) Windows Server(R) 2003
           Microsoft(R) Windows Server(R) 2008
           Microsoft(R) Windows Vista(R)
           Microsoft(R) Windows(R) 7

     <2> To specify custom paper size in a cluster environment, specify a
         common setting for all physical nodes in the cluster environment. 

     <3> When [Search Printer] dialog box appears at the press of the [Get
         Information from Printer] button, enter the printer network
         address. 

     <4> Deleting driver in cluster environment
         (A) Microsoft(R) Windows Server(R) 2000
             After the driver on the virtual server is deleted, delete the
             drivers on all standby nodes. 

         (B) Microsoft(R) Windows Server(R) 2003 or Microsoft(R) Windows
             Server(R) 2008
             After the driver on the virtual server is deleted, delete the
             drivers on all standby nodes. 
             ** Deleting driver from the standby node
             (b-1) Change the standby node to active node. 
             (b-2) Install printer on virtual server. 
             (b-3) Delete driver from virtual server. 

     <5> Deleting driver
         After the printer icon is deleted, delete the driver from [Server
         Properties].  Then, restart the computer. 

(18) [Cancel] button on [User Details Setup] Dialog
     For some applications, if [Enter User Details] dialog is cancelled 
     when printing with the settings of [Prompt User for Entry when Submitting 
     job] on [User Details Setup] dialog, a warning dialog may be displayed.  
     This warning dialog may indicate a printer error, however, the printer 
     actually has no problem.

     In that case, ignore the warning and continue.

(19) Functional Limitations of EMF Spooling
     When [EMF Spooling] of [Advanced Settings] tab is set to Enabled, the following 
     features may not function normally.
     To use these features, set [EMF Spooling] to Disabled.
     *[Secure Print][Sample Set][Delayed Print][Save to Mailbox]
     *[Enable Account Setup] [User Details Setup]
     *[Notify Job Completion by E-mail]
     *[Annotation]
     *[Create / Register Forms]
     *[Insert Separators] of [Covers / Separators]
     *[ICM Adjustment] of [Image Adjustment Mode]
     *[Use Extended Features From Application]
     *[Enable User Defined Margins]
     *All features of Direct Fax Driver

     When [EMF Spooling] of [Advanced Settings] tab is set to Disabled, some documents 
     with complex structure may have troubles such as distorted output image and failure of 
     the output.
     In Windows Vista(R) environment, documents can be output normally.
     Also in Windows(R) XP and Windows Server(R) 2003 environments, documents can be output 
     normally by applying SP2.

(20) To change the settings of Custom Paper Size, you need the Administrator's 
     access rights.

     On Windows Vista(R), select printer from the printer folder, right-click to go
     [Run as administrator] and select [Properties].  After clicking [Continue] in
     [User Account Control], you can change the settings from Property.

     On Windows 7, Windows Server 2008 R2, Windows 8 or Windows Server 2012, 
     select a printer from the [Devices and Printers] folder.
     Select Property of the printer and click the "Change Sharing Options" 
     button on the "Sharing" tab.
     Then, specify Custom Paper Size.

(21) With the default settings of Firewall on Windows Vista,
     Windows Server 2008, Windows 7, Windows Server 2008 R2, Windows 8 or
     Windows Server 2012, data in cross-subnet broadcast cannot be retrieved.
     For cross-subnet data retrieval, please do not use broadcast and specify
     address directly.

(22) There are feature restrictions below on the execution of Fax print in 
     Protected Mode of Internet Explorer on Windows Vista(R).
     - A warning message may be displayed right after the execution of Fax print.
     - The location for storage of Fax Phonebook is not a Public Folder, 
       which is usually used for storage but a folder such as personal Folder, 
       which can be used for file creation.  Therefore, the contents of Fax Phonebook
       are different from the one registered with other applications.
     - Import To List feature of Fax Phonebook does not function.

(23) There is a restriction in creating file from Internet Explorer in
     Windows Vista(R). You cannot save form data file in the folder specified as
     the default in "Create / Register Forms". Change the folder into one
     that can be used for creating file (such as "Document Folder") before
     creating/registering form data file.

(24) Watermarks features
     In Windows(R) XP SP2, Windows Server(R) 2003 SP2, Windows Server(R) 2008 and 
     Windows Vista(R) environments, when [EMF Spooling] of [Advanced Settings] tab
     is set to disabled, [Watermarks] is not available for use by 32bit application
     software.  To use this feature, set [EMF Spooling] to Enabled.

(25) Annotation Options features
     In Windows(R) XP SP2, Windows Server(R) 2003 SP2 and Windows Vista(R) environments, 
     when [EMF Spooling] of [Advanced Settings] tab is set to Disabled, [Annotation] 
     is not available for use by 32bit application software.  
     To use this feature, set [EMF Spooling] to Enabled.

(26) The remote installation of a print driver from the Print Server to Windows Vista(R)
     or later may not complete normally.  It is recommended that you perform the remote
     installation on Windows(R) XP.


6. Software Update
==================
    The latest software is available on our web site.

        http://www.fxap.com.sg/default.jsp

    Communication charges will be borne by the customer.


Portions of this software are based in part on the work of the
Independent JPEG Group.

Microsoft is the registered trademark of Microsoft Incorporated.
Windows is the registered trademark of Microsoft Incorporated.
Other names of products and companies are the trademarks or
registered trademarks of each company.
(C) Fuji Xerox Co., Ltd. 2004-2012
----------------------------< End of File >--------------------------

